**Step-by-Step Guide to Set-up Raspbian Stretch**

Disclaimer: Note that the Raspberry Pi Zero – although running Raspbian Stretch as all other Raspberry Pi’s – is ARMv6 architecture in contrast to the most common ARMv7 architecture as used on the Raspberry Pi 3. However, all steps described in this guide should work on both and were tested on a Raspberry Pi Zero W.

Before you begin, check your default python version with:

* pi@raspberrypi:~$ python --version

This guide is written for python 2.7 and assumes it is the default python-compiler on the target system. All steps were performed under afore-mentioned conditions and systems only. Apart from this, it is highly recommended that all **pip**-installs are run as follows:

* Instead of: pi@raspberrypi:~$ ~~pip install numpy~~
* Better run: pi@raspberrypi:~$ python -m pip install numpy

This will install the package more specific to your default-compiler and showed advantages relating dependencies-setup.

1. Browse to: <https://www.raspberrypi.org/downloads/raspbian/>
2. Download Raspbian Stretch
3. Flash it to Micro-SD-Card with at least 8GB capacity (e.g. with Etcher on Windows)
4. Set up your WiFi-Connection if not already done
5. *Optional*: First get packagelist with package size and then get rid of unnecessary packages in order to free some space on your SD-Card:

* pi@raspberrypi:~$ dpkg-query -Wf '${Installed-Size}\t${Package}\n' | sort -n
* pi@raspberrypi:~$ sudo apt-get remove --purge wolfram-engine
* pi@raspberrypi:~$ sudo apt-get clean
* pi@raspberrypi:~$ sudo apt-get autoremove

1. Install Kivy for Raspbian Stretch ( according to <https://kivy.org/docs/installation/installation-rpi.html> ):

* pi@raspberrypi:~$ sudo apt-get update
* pi@raspberrypi:~$ sudo apt-get install libsdl2-dev libsdl2-image-dev libsdl2-mixer-dev
* pi@raspberrypi:~$ sudo apt-get install libsdl2-ttf-dev pkg-config libgl1-mesa-dev
* pi@raspberrypi:~$ sudo apt-get install libgles2-mesa-dev python-setuptools libgstreamer1.0-dev
* pi@raspberrypi:~$ sudo apt-get install git-core gstreamer1.0-plugins-{bad,base,good,ugly}
* pi@raspberrypi:~$ sudo apt-get install gstreamer1.0-{omx,alsa} python-dev libmtdev-dev
* pi@raspberrypi:~$ sudo apt-get install xclip xsel
* Install Kivy globally on your system but with the following command

1. Install Cython 0.28.3 ( according to <https://kivy.org/docs/installation/installation-rpi.html> ):

* pi@raspberrypi:~$ sudo python -m pip install -U Cython==0.28.3 (takes approx. 2h on RasPi Zero)

1. Install Kivy ( according to <https://kivy.org/docs/installation/installation-rpi.html> ):

* pi@raspberrypi:~$: sudo pip install git+https://github.com/kivy/kivy.git@master

(takes approx. 2h on RasPi Zero)

1. Open RasPi Config and activate SSH:

* pi@raspberrypi:~$ sudo raspi-config
* Navigate to: Interfacing Options ⇨ SSH ⇨ Enable SSH ⇨ Yes

1. Connect to your Raspberry Pi using its IP-Address within your Network (e.g. with PuTTy on Windows
2. Create Folder “Programming” in home directory. Change into that folder via SSH-Terminal
3. Fetch FludiscopeApp from Benedict Diederichs Branch on GitLab:

* pi@raspberrypi:~$ git clone -b developBD --single-branch git@gitlab.com:renerichter/PPS-app.git

1. Browse to: ~/Programming/PPS-app/code/
2. Run: python main.py
3. Install all missing dependencies you are notified about to be missing (list may be incomplete):

* pi@raspberrypi:~$: python -m pip install unipath
* pi@raspberrypi:~$: python -m pip install ruamel.yaml
* pi@raspberrypi:~$: sudo apt-get install libffi-dev
* pi@raspberrypi:~$: python -m pip install cffi
* pi@raspberrypi:~$: python -m pip install smbus-cffi
* pi@raspberrypi:~$: python -m pip install pyusb
* pi@raspberrypi:~$: python -m pip install safe-cast

1. Install pre-compiled OpenCV 2.4.9.1 as described in order to save hours of compile-time as opposed to widespread conventional install. Get OpenCV-dependencies in advance. And check it installed correctly afterwards.

* pi@raspberrypi:~$: sudo apt-get update
* pi@raspberrypi:~$: sudo apt-get upgrade
* pi@raspberrypi:~$ sudo apt-get install libtiff5-dev libjasper-dev libpng12-dev
* pi@raspberrypi:~$ sudo apt-get install libjpeg-dev
* pi@raspberrypi:~$ sudo apt-get install libavcodec-dev libavformat-dev libswscale-dev libv4l-dev
* pi@raspberrypi:~$ sudo apt-get install libgtk2.0-dev
* pi@raspberrypi:~$ sudo apt-get install libatlas-base-dev gfortran
* pi@raspberrypi:~$ sudo apt-get install libopencv-dev python-opencv python-picamera
* pi@raspberrypi:~$ python
* >>> cv2.\_\_version\_\_

1. Enable I2C, Serial Communication and PiCamera:

* pi@raspberrypi:~$: sudo raspi-config

1. *Optional [RasPi 3]*: Install TeamViewer for remote maintenance:

* pi@raspberrypi:~$: sudo apt-get update && sudo apt-get dist-upgrade
* pi@raspberrypi:~$: wget <http://download.teamviewer.com/download/linux/version_11x/teamviewer-host_armhf.deb>
* pi@raspberrypi:~$: sudo dpkg -i teamviewer-host\_armhf.deb (will throw some errors, that’s okay)
* pi@raspberrypi:~$: sudo apt-get -f install (will fix previous errors)

1. *Optional [RasPi Zero W]*: Install TeamViewer for remote maintenance:

* pi@raspberrypi:~$: sudo nano /etc/dphys-swapfile

1. das
2. das
3. das
4. das
5. das
6. das
7. das
8. das
9. da